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Queensberry Street Riding lanes
Peel Street to Rathdowne Street
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[bookmark: _Toc169617296]Peel Street to Rathdowne Street
Prior to Metro Tunnel works starting, Queensberry Street had one traffic lane in each direction.
With Grattan Street now open and Metro Tunnel’s new Parkville Station almost complete, we’re proposing to reinstate Queensberry Street to one traffic lane in each direction, and deliver safer and better-connected riding lanes from Peel Street to Rathdowne Street.
In line with City of Melbourne’s Urban Forest Strategy, we’re also proposing to plant up to 57 trees. This mix of small to large evergreen and deciduous trees will help to create a cooler environment in the warmer months, reduce air pollution, encourage outdoor activity and support biodiversity.
[bookmark: _Toc169617297]Details of treatments for this project
Protection at intersections[image: Cyclists lined in a riding lane next to a waiting truck separated by a raised concrete separator island ]
[bookmark: _Toc403992348][bookmark: _Toc403992583]Flexible bollard [image: Green flexible bollard in front of a raised concrete island]
Concrete separator kerbs [image: Raised narrow concrete island]
Concrete separator islands[image: A raised concrete island with granitic sand infill]
Footpath extensions[image: A footpath that has been extended into the roadway at an intersection]
Island with tree planting [image: A grassed traffic island with trees planted in it.  It is location between a riding lane and parked cars]
Vehicle hook turn boxes [image: An intersection showing queued cars in a hook turn box]
Green surface treatment at selected locations[image: Green surface treatment with a bike logo]
[bookmark: _Toc169617298]Road cross-sections
Previous conditions on Queensberry Street [image: Previous conditions show road cross-section with trees and parking in the middle of the road and a single traffic lane with parking and a riding lane in each direction]

Existing conditions on Queensberry Street[image: Existing layout shows a road cross-section with a tree in the median and two traffic lanes, parking and a riding lane in each direction]
Proposed new conditions on Queensberry Street [image: Proposed Layout shows a protected bike lane, a new island with trees, parking and a single traffic lanes in each direction .]
Map of the surrounding riding lane network[image: Map of the works area and riding lanes in the surrounding streets]
[bookmark: _Toc169617299]Queensberry Street Riding Lanes (1/4)
Section: Peel Street to Leicester Street
Key changes:
Reduced traffic lanes in both directions. 
Protected riding lanes on both sides of the street, and on Leicester and Bouverie Streets approaching Queensberry Street.
Green surface treatment at selected locations.
Up to 4 new trees.
New zebra crossings on O’Connell and Berkeley Streets.
Wider footpaths on the corners of O’Connell, Berkeley and Leicester Streets with new trees.
Right turn traffic bans at O’Connell and Berkeley Streets.
Hook turn boxes at Elizabeth Street (eastbound) and Leicester Street.
14 parking bays retained (12 removed).
[image: Queensberry between Peel and Leicester Street
Plans showing the layout of the proposed street with protected riding lanes, intersections, new footpath extension and new trees]
[bookmark: _Toc169617300]Queensberry Street Riding Lanes (2/4)
Section: Swanston Street to Lygon Street
Key changes: 
Reduced traffic lanes in both directions. 
Protected riding lanes on both sides of the street. 
Green surface treatment at selected locations. 
Up to 20 new trees. 
Gaps closed in median islands to improve safety. 
Hook turn boxes at signalised intersections. 
31 parking bays retained (14 removed). 
[image: Queensberry between Leicester and Swanston Street.
Plans showing the layout of the proposed street with protected riding lanes, intersections, new footpath extension and new trees]
[bookmark: _Toc169617301]Queensberry Street Riding Lanes (3/4)
Section: Swanston Street to Lygon Street
Key changes: 
Reduced traffic lanes in both directions. 
Protected riding lanes on both sides of the street. 
Green surface treatment at selected locations. 
Up to 20 new trees. 
Gaps closed in median islands to improve safety. 
Hook turn boxes at signalised intersections. 
31 parking bays retained (14 removed). 
[image: Queensberry between Swanston and Rathdowne Street.
Plans showing the layout of the proposed street with protected riding lanes, intersections, new footpath extension and new trees]
[bookmark: _Toc169617302]Queensberry Street Riding Lanes (4/4)
Section: Lygon Street to Rathdowne Street
Key changes: 
Reduced traffic lanes in both directions. 
Protected riding lanes on both sides of the street. 
Green surface treatment at selected locations. 
Up to 13 new trees. 
Gaps closed in median islands to improve safety. 
Hook turn boxes at signalised intersections. 
[image: Queensberry St between Lygon St and Rathdowne St.
Plans showing the layout of the proposed street with protected riding lanes, intersections, new footpath extension and new trees]
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Queensberry Future - Proposed
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